**PRIZM RX Connection**

**Nov 25 2016**

If the PRIZM is used to give power to the RX, then Servo Motors cannot be plugged into the RX, they must be plugged into the PRIZM pwm slots.

If the RX is read by an Analog Pin from the PRIZM, then the power to the RX must be provided by the PRIZM.

If you use a Limit Switch with the PRIZM, you must use a large enough resistance such as 300 K ohm.

Si le PRIZM donne le power au receiver aucun servos peuvent être branché dans le receiver, ils doivent être branché dans le PRIZM

Si le receiver est lu par une pin analog, le power au receiver dois être fourni par le PRIZM

Si tu utilise une limit swich avec le PRIZM, tu dois utiliser une résistance de 0.3 M ohm ou 300 k ohm sinon on va court-circuiter la « board ».